Interface Ethernet 0/0/0 on router 3 which is connected to router 4 is configured as passive interface hence router 3 Ethernet interface not sending updates on that interface.

Remove the passive interface restriction on Ethernet 0/0/0 of router 3; you will be able to see Rip routes on router 4