Switch1 is configured with VTP transparent mode.

Transparent mode ignores all VTP updates; change the VTP mode to either server or client to solve the issue.