Interface FA 0/24 on switch that is connected to router is configured as Access port, change the interface to trunk so that switch can pass Vlan tagged traffic to the switch.