VTP domain on switch1 is different than the other switches.

Configure same VTP domain on switch1 to solve the issue.