EIGRP process ID is not matched for the routers. EIGRP process ID should be same on routers to form the neighbor relationship.

Match the EIGRP process ID on both routers to successfully configure the neighbor relationship.