Access list is configured correctly however it is applied on the wrong interface which is preventing traffic to enter router 3.

Apply the access list to the interface FA 0/0 of router 3 to only block access to 192.168.2.2 host.